**Addendum #1**

**Harmon Field Snack Shack Project**

Dated April 24, 2019

*Prepared by Brenda Day, Administrative Assistant and Jeff Frey, Clerk of the Works*

1. The front roof overhang shall be framed to provide a soffit square  
from the building. Prior to the installation of soffit finish  
materials, the owner shall be provided reasonable notice to allow the  
installation of any blocking, wiring and/or light fixtures. This  
change will enhance the appearance of the existing overhang as well as  
provide additional structure integrity to the structure.  
  
  
2. Proposed second floor fixed glass window will instead become an  
opening with removable shutter to provide cross ventilation and  
provide better sightline when opened. Shutter and framed casing shall  
be constructed to be weather tight when closed. A sketch submittal  
shall be required for approval prior to construction.  
  
  
3. Exterior stair landing. Provide a 24" deep by 6" thick poured  
concrete slab the width of the stairs to serve as the stair landing.  
Slab to provide broom finish and edge troweled.