**Addendum #1**

**Harmon Field Snack Shack Project**

Dated April 24, 2019

*Prepared by Brenda Day, Administrative Assistant and Jeff Frey, Clerk of the Works*

1. The front roof overhang shall be framed to provide a soffit square
from the building. Prior to the installation of soffit finish
materials, the owner shall be provided reasonable notice to allow the
installation of any blocking, wiring and/or light fixtures. This
change will enhance the appearance of the existing overhang as well as
provide additional structure integrity to the structure.

2. Proposed second floor fixed glass window will instead become an
opening with removable shutter to provide cross ventilation and
provide better sightline when opened. Shutter and framed casing shall
be constructed to be weather tight when closed. A sketch submittal
shall be required for approval prior to construction.

3. Exterior stair landing. Provide a 24" deep by 6" thick poured
concrete slab the width of the stairs to serve as the stair landing.
Slab to provide broom finish and edge troweled.